## CD Review Results, Verification Plan and Field Verified Results

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | CD Review Results | | Verification Plan | | | Field Verification Results | |
| Measure | Description | CD Review | Verification Approach | Short-Term Data Logging | Long-Term Data Logging | Verification Status | Notes |
| 20% EPD Reduction in Guest Rooms Only | Reduce EPD in guest rooms with EnergyStar rated TVs and mini-fridges. | Only a 15% EPD reduction was found in guest rooms. Mini-fridges were EnergyStar rated but not TVs | Determine EPD in guest rooms by sampling rooms and counting equipment power | None | None | Verified | EnergyStar TVs were installed; model 20% EPD reduction |
| 20% LPD Reduction in Guest Rooms Only | Reduce LPD in guest rooms with CFLs and vacancy sensors | Found as modeled | Count fixtures and inspect lamp and ballast ratings. | Put data logger in guest rooms to verify vacancy sensor operation | None | Verified |  |
| R-15 Exterior Wall Insulation Only | R-15 exterior walls | Found as modeled | Review installation | None | None | Verified |  |
| R-50 Roof Insulation Only | R-50 roof insulation | Only R-45 insulation was found in the roof construction. | Review installation | None | None | Verified | R-40 Roof insulation installed; model R-40 Roof insulation |
| Rotate Building 90 Degrees Only | Building sited with long axis E-W | Found as modeled | Visit building site ☺ | None | None | Verified |  |